TankBot Building Instructions 1 2

3 4

1x16 beam black connector peg

4x 4x

make 2 of these

black pegs act as rivets to hold beams together axle 4x full bushing 8x 1st hole from left

3rd hole from right

full bushing

24 tooth gear

2x 2x

make sure these axles can spin freely

2x8 plate 4x

double-wide beams and plates give the chassis added strength

TankBot Building Instructions 6 2x8 plate 2x 5^{2x2 brick 2x4 plate 1x4 plate}

4x 2x 2x

7^{motor}

2x

8 2x

24 tooth gear

Do the same on the other side

TankBot Building Instructions

2x8 plate

2x 9 10

11 12

black connector peg

4x

3rd hole from left 8th hole from left Do the same on both sides

short brown connector peg RCX

4x 1x

Insert short end into RCX Do the same on both sides

1x8 beam

4x

These crossbraces hold the RCX securely to the robot’s body.

Do the same on both sides.

TankBot Building Instructions

white hub full bushing 16 tooth gear

tread short motor cable

13

14 15

4x 2x 2x

2x 2x

16 tooth gear

Do the same on both sides

Do the same on both sides

Connect the cables exactly as shown